{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["IO MAP"],"not_rendered":{"images":1},"read":"whole","date_system":"1900"}

{"sheet":"IO MAP","index":0,"n_rows":54,"n_cols":14,"rows_kept":54,"merged":[[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,9,2,9],[1,10,2,10],[1,11,2,11]]}
[]
[null,"No","Name","PAD type","defualt",0,1,2,3,"ANA func","PAD connect","备注"]
[{"$nulls":5},"GPIO","CSC func","special","GPTIM ",{"$nulls":4},"ADC语音示意图,  电阻和电容需要根据咪头确定"]
[null,1,"PADA0","IO RT25","SWCLK，PULLDOWN","PA00","CSC","SWCLK",null,"ADCIN0"]
[null,2,"PADA1","IO RT25","SWDIO，PULLUP","PA01","CSC","SWDIO","CTMR_ETR_IN(I)","ADCIN1"]
[null,3,"PADA2","IO RT25","GPIO","PA02","CSC",null,"CTMR_CH1(I/O)","ADCIN2","MICBIAS"]
[null,4,"PADA3","IO RT25","GPIO","PA03","CSC",null,"CTMR_CH2(I/O)","MICIN"]
[null,5,"PADA4","IO RT25","GPIO","PA04","CSC","DPLL_LOCKED(O)","CTMR_CH3(I/O)","ADCIN3"]
[null,6,"PADA5","IO RT25","GPIO","PA05","CSC","CLK_OUT(O)","CTMR_CH4(I/O)","ADCIN4"]
[null,7,"PADA6","IO RT25","GPIO，PULLUP","PA06","CSC",null,"ATMR_BK(I)","ADCIN5","DP","Uart烧录 Tx"]
[null,8,"PADA7","IO RT25","GPIO，PULLUP","PA07","CSC",null,"ATMR_CH1P(I/O)","ADCIN6","DM","Uart烧录 Rx"]
[null,9,"PADA8","IO RT25","GPIO","PA08","CSC",null,"ATMR_CH2P(I/O)","ADCIN7"]
[null,10,"PADA9","IO RT25","GPIO","PA09","CSC","USB_DOP(O)","ATMR_CH3P(I/O)","ADCIN8"]
[null,11,"PADA10","IO RT25","GPIO","PA10","CSC","USB_DOM(O)","ATMR_CH4P(I/O)","ADCIN9"]
[null,12,"PADA11","IO RT25","GPIO","PA11","CSC","USB_NDOE(O)","ATMR_CH1N(O)","ADCIN0"]
[null,13,"PADA12","IO RT25","GPIO","PA12","CSC",null,"ATMR_CH2N(O)","ADCIN1"]
[null,14,"PADA13","IO RT25","GPIO","PA13","CSC",null,"ATMR_CH3N(O)","ADCIN2"]
[null,15,"PADA14","IO RT25","GPIO","PA14","CSC",null,"ATMR_ETR_IN(I)","ADCIN4"]
[null,16,"PADA15","IO RT25","GPIO","PA15","CSC",null,"CTMR_CH1(I/O)","ADCIN5"]
[null,17,"PADA16","IO RT25","GPIO","PA16","CSC",null,"CTMR_CH2(I/O)","ADCIN6"]
[null,18,"PADA17","IO RT25","GPIO","PA17","CSC",null,"CTMR_CH3(I/O)"]
[null,19,"PADA18","IO RT25","GPIO","PA18","CSC",null,"CTMR_CH4(I/O)"]
[null,20,"PADA19","IO RT25","PULLUP，nRESET","PA19","CSC"]
[]
[]
[]
[]
[]
[]
[null,"csc_fout_sel0",null,"UART1_TXD(IO)",0,{"$nulls":3},"csc_fin_sel0","UART1_TXD(IO)",0]
[null,"csc_fout_sel1",null,"UART1_RXD(IO)",1,{"$nulls":3},"csc_fin_sel1","UART1_RXD(IO)",1]
[null,"csc_fout_sel2",null,"UART2_TXD(IO)",2,{"$nulls":3},"csc_fin_sel2","UART2_TXD(IO)",2]
[null,"csc_fout_sel3",null,"UART2_RXD(IO)",3,{"$nulls":3},"csc_fin_sel3","UART2_RXD(IO)",3]
[null,"csc_fout_sel4",null,"I2C_SCL(IO)",4,{"$nulls":3},"csc_fin_sel4","I2C_SCL(IO)",4]
[null,"csc_fout_sel5",null,"I2C_SDA(IO)",5,{"$nulls":3},"csc_fin_sel5","I2C_SDA(IO)",5]
[null,"csc_fout_sel6",null,"CTMR_CH1(IO)",6,{"$nulls":3},"csc_fin_sel6","CTMR_CH1(IO)",6]
[null,"csc_fout_sel7",null,"CTMR_CH2(IO)",7,{"$nulls":3},"csc_fin_sel7","CTMR_CH2(IO)",7]
[null,"csc_fout_sel8",null,"UART1_RTS(O)",8,{"$nulls":3},"csc_fin_sel8","UART1_CTS(I)",8]
[null,"csc_fout_sel9",null,"UART2_RTS(O)",9,{"$nulls":3},"csc_fin_sel9","UART2_CTS(I)",9]
[null,"csc_fout_sel10",null,"UART1_SCK(O)",10,{"$nulls":3},"csc_fin_sel10","SPIM_MISO(I)",10]
[null,"csc_fout_sel11",null,"UART2_SCK(O)",11,{"$nulls":3},"csc_fin_sel11","SPIS_CLK(I)",11]
[null,"csc_fout_sel12",null,"SPIM_CLK(O)",12,{"$nulls":3},"csc_fin_sel12","SPIS_MOSI(I)",12]
[null,"csc_fout_sel13",null,"SPIM_MOSI(O)",13,{"$nulls":3},"csc_fin_sel13","SPIS_CSN(I)",13]
[null,"csc_fout_sel14",null,"SPIS_MISO(O)",14]
[null,"csc_fout_sel15",null,"GLB_BIST_DONE(O)",15]
[null,"csc_fout_sel16",null,"GLB_BIST_FAIL(O)",16]
[null,"csc_fout_sel17",null,"OSCEN_FLG(O)",17]
[null,"csc_fout_sel18",null,"RFEN_FLG(O)",18]
[null,"csc_fout_sel19",null,"BLE_SLEEP_FLAG(O)",19]
[null,"csc_fout_sel20",null,"CM0P_DEEPSLEEP(O)",20]
[null,"csc_fout_sel21",null,"BB_TX_EN(O)",21]
[null,"csc_fout_sel22",null,"BB_RX_EN(O)",22]
[null,"csc_fout_sel23",null,"MDM_TX_EN(O)",23]
[null,"csc_fout_sel24",null,"MDM_RX_EN(O)",24]